The VEKA system with the classic design

Product description

* 5-chamber profile with 70 mm basic installation depth
* Insulation values of up to Uw = 0.76 W/(m²K) when using highly insulating triple glazing with Ug 0.4 W/(m²K)
* Classic contours with slightly rounded edges, particularly small visible surfaces and grey seals
* Particularly low maintenance thanks to homogeneous surfaces and surface-flush glazing beads
* Optimal stability for long-lasting functionality and value retention
* Total compatibility with the other VEKA 70 mm systems SWINGLINE and TOPLINE
* Available as recessed and semi-recessed version
* Also suitable for the manufacture of parallel slide & tilt doors