The VEKA system that is ready for future requirements

Product description

* 82 mm system with innovative multi-chamber geometry for excellent thermal insulation
* Insulation values of up Uw = 0.67 W/(m²K) when using highly insulating triple glazing with Ug 0.4 W/(m²K)
* Glass penetration of 25 mm reduces heat transfer
* Universally suitable for new constructions and house renovation projects
* Wall thickness at the highest RAL quality standard ‘Class A’ (DIN EN 12608)
* Three-level seal keeps out noise, cold, damp and draughts
* Also available as AD system with rebate seal
* Surface finishing with films and skirtings possible