The VEKA system that is ready for future requirements

Product description

* 82 mm system with innovative multi-chamber geometry for excellent thermal insulation
* Insulation values of up Uw = 0.71 W/(m²K) when using highly insulating triple glazing with Ug 0.4 W/(m²K)
* 28 mm glazing rebate reduces the number of thermal bridges
* Very easy to clean due to the flat surface between the sash and the frame
* Classic design and unpretentious look
* Can be used for any new construction or renovation
* Highest VEKA class A quality with wall thicknesses in accordance with DIN EN 12608
* Surface can be upgraded with film and a cover